**Figure 3. Areas under the receiver-operator and precision-recall curves**

